Is the device up?

Device is down

Device is up

Ping

YES = 0 NO = 0